|  |  |
| --- | --- |
| Exp 1. Common Emitter Amplifier | Section 1.6.1. Bias Measurements |
| Tom Brewer | Collector Voltage = 7.28 V  Base Voltage = 2.07 V  Emitter Voltage = 1.42 V  Collector Current =(15‐7.28)/10k=0.773 mA |
| Section 1.6.2. Small Signal Gain Gain=651/14.1=46.2 | Section 1.6.3. Frequency Response |
|  |  |
| Section 1.6.3. Frequency Response | Section 1.64. Large‐Signal Clipping Behavior |
| From Bode Plot:  Midband Gain (dB)=‐0.9+20log(1020/20)=33.25 Midband Gain (linear)=46  Lower 3db= 66Hz  Upper 3db=360k |  |